The loudspeaker shall be a 2-way passive short throw point source system. The low-mid frequency range shall be reproduced by a couple of direct radiating 6” transducers. The high frequency range shall rely on one 2” VCD compression driver coupled to a constant directivity rotatable horn. The enclosure shall be manufactured from premium Baltic birch plywood and finished with polyurea paint (CX) or fiberglass (DX) for direct exposure applications. The enclosure front shall be protected by a coated stainless steel grill and an triple layer mesh including hydrophobic fabric. The enclosure shall incorporate M10 rigging points to be used for permanent installation.
The loudspeaker shall be EN-54-24 certified.
Performance specifications for a typical production unit shall be as follows, measured at 1/3-octave resolution: operating frequency range (-10dB) 70 Hz to 22 kHz.
Horizontal nominal coverage (-6dB): 80º
Vertical nominal coverage (-6dB): 80º 
On-Axis Sensitivity (1W/1m): 93dB
Maximum Peak SPL:  122dB 
Dimensions shall be (H x W x D) 54.5 x 22.6 x 26.7 cm (21.5 x 8.9 x 10.5 in). Weight shall be 12 kg (26.4 lbs). The loudspeaker shall be the DAS Audio WR-8826.


