Extracting The Library:
Britex ArchiCAD libraries are compiled in Library Container Files (.lcf). The LCF contains the GDL Object files (.gsm) and a folder of the product images utilised in the Graphical User Interface. If, for any number of reasons, you decide to extract the LCF files (File menu > Libraries and Objects > Extract a Container) you need to ensure when you reload the extracted GDL Object files into ArchiCAD that you include the necessary image files for that object as well as the Britex (and Rubysketch) logo image files. For your convenience the image files for each Britex GDL Object have been group into their own sub folders within the LCF file.
 
Editing GDL Script
If you edit the scripting of any Britex GDL Objects you must be aware that all scripting is intelligently linked and editing carelessly may cause error messages.
